"Symbol";"Value";"Unit";
"REFERENCE";"EC-2M-12";"";
"TraceParts.PartVersion";"1.2.2";"";
"SUPPLIER";"Clippard Minimatic";"";
"TraceParts.PartStatus";"Published";"";
"TraceParts.PartNumber";"10-29102010-105096";"";
"TraceParts.PartLanguage";"en";"";
"DESIGN";"2-Way Normally-Closed Valves, Manifold Mount - Standard - 0,025 Pin Connector - Vac. to 105 psig+ - 12 VDC";"";
"TraceParts.InstanceId";"10-29102010-1050969N0ZT0SNH54M5MXX9IBLQSDSM";"";
"TraceParts.PartTitle";"Electronic EV Series Mouse Valves - 2-Way Normally-Closed - Standard";"";
"OMNICLASS23";"23.27.33.11.11";"";
"TRACEPARTS";"TRACEPARTS";"";
"TraceParts.PartStatusId";"";"";
"TraceParts.ClassPath";"CLIPPARD:10-29102010-105096";"";
