Included in this folder are models of Clippard pneumatic components.

* UDR-17-6: pneumatic cylinder actuator, 1 1/16", universal mount, rotating rod, double-acting, 6" stroke
udr-17-6.SLDASM
udr-17-6_01.SLDPRT
udr-17-6_02.SLDPRT

minimum axis to axis distance roughly 275 mm
travel roughly 150 mm
maximum axis to axis distance roughly 435 mm

* UDR-17-3: pneumatic cylinder actuator, 1 1/16", universal mount, rotating rod, double-acting, 3" stroke
udr-17-3.SLDASM         
udr-17-3_01.SLDPRT      
udr-17-3_02.SLDPRT      
udr-17-3.txt

* CDR-24-6: pneumatic cylinder actuator, 1 1/2", universal mount, rotating rod, double-acting, 6" stroke
cdr-24-6.SLDASM         
cdr-24-6_01.SLDPRT      
cdr-24-6_02.SLDPRT      
cdr-24-6.txt            

* RC-1781: rod clevis assembly, 1 1/16" Bore Size
rc-1781.SLDASM
rc-1781.txt
rc-1781_01.SLDPRT
rc-1781_02.SLDPRT
rc-1781_03.SLDPRT

* EFB-2M: fill & bleed circuit, manifold only
efb-2m.SLDPRT

* MMM-41-02: 2-station manifold for 4-way MME/MMA-41 series valves
MMM-41-02-manifold.SLDPRT

* EC-PM-10-25A0: proportional valve
valve_ec-pm-10-25a0.SLDPRT

* 15481-4: 4-station manifold
manifold_15481-4.SLDPRT

